501 Innovative Way | Zebulon, NC 27597 | NOMACO.COM



**Specifying NOMAFLEX® by Nomaco, Inc.**

Typically placed in the following MasterFormat Specification Sections: Section 03 30 00 – CAST-IN-PLACE CONCRETE.

Section 32 13 13 – CONCRETE PAVING

# PART 2 PRODUCTS

* 1. **JOINT MATERIALS**
		1. Joint Filler: Preformed Expansion Joint Filler or Slab Isolation Joint Filler with typical thickness 1/2, 3/4, or 1 inch and height equal to slab thickness. May be specified with or without a removable top section for creation of a sealant void.
			1. Materials: Provide a semi-rigid, closed-cell polypropylene foam, preformed joint filler that fully complies with ASTM D8139. NOMAFLEX® by Nomaco, Inc.
			2. Manufacturers: Nomaco, Inc., 501 Innovative Way, Zebulon, NC 27597. Phone (877) 291-1157. Fax (919) 269-7936. Website: <https://www.nomaco.com/product/nomaflex/>

Specifier Notes: Specify the thickness of the expansion-isolation joint filler and sealant void creation option if desired.